{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":21,"n_cols":7,"rows_kept":21,"flags":["formulas_cached_only"]}
["8000吨/年高活性结晶级聚苯硫醚树脂数智化生产线示范项目（一期4000吨/年）物资需求清单（第一批）"]
["序号","名称","技术参数、规格型号","单位","数量","备注说明","采购方案"]
[1,"仪表切断阀","详细数据表见附件1","台",1,"放料罐溶剂冲洗阀","询比"]
[2,"仪表切断阀","详细数据表见附件2","台",2,"进1R11~1501A~D DCB管线","询比"]
[3,"仪表切断阀","详细数据表见附件2","台",2,"进1R11~1501A~D NMP管线","询比"]
[4,"仪表切断阀","详细数据表见附件3","台",2,"1V11~1503A~D排水管线","询比"]
[5,"仪表切断阀","详细数据表见附件3","台",1,"进1V11~1503A~D氮气管线","询比"]
[6,"仪表切断阀","详细数据表见附件4","台",1,"1M3(101-501)半成品离心机进料开关阀","询比"]
[7,"仪表切断阀","详细数据表见附件4","台",1,"1V31（5）02半成品高位槽进料开关阀","询比"]
[8,"调节阀","详细数据表见附件5","台",1,"1V1509底部出料","询比"]
[9,"调节阀","详细数据表见附件5","台",1,"1V1510底部出料","询比"]
[10,"在线液位计","详细数据表见附件6","台",3,"脱水液计量液位","询比"]
[11,"涡街流量计","详细数据表见附件7","台",1,"1V1109 NMP高位槽下部出料流量","询比"]
[12,"电磁阀","详细数据表见附件8","台",3,"阀门配套电磁阀","询比"]
[13,"DCS系统卡件","详细数据表见附件9","套",1,"中控系统","询比"]
[14,"加料斗（盖板）","1.材质：316L不锈钢，厚度≥5mm；\n2.容积：适配现有加料口尺寸，容积≥50L；\n3.结构：带密封盖板，防止粉尘泄漏与物料受潮；\n4. 接口：与现有加料手阀精准匹配，安装稳固。","个",3,"现场测量后加工制作","询比"]
[15,"视镜","1.公称直径：DN40；\n2.视镜材质：硼硅玻璃，抗压强度≥1.0MPa；\n3.外壳材质：316L不锈钢，耐腐蚀；\n4. 安装方式：法兰连接，便于拆卸更换。","个",3,"脱水液","询比"]
[16,"视镜","1.公称直径：DN40；\n2.视镜材质：硼硅玻璃，透光率≥95%；\n3.外壳材质：316L不锈钢；\n4.工作压力：≥0.6MPa，工作温度：≤200℃；\n5. 密封形式：PTFE垫片，无泄漏。","个",3,"脱水计量槽出口","询比"]
[17,"直线筛","详见附件11--请购文件","台",1,null,"询比"]
[19,"压滤泵","详见附件12--请购文件","台",2,null,"询比"]
[20,"粉碎上料机","详见附件10--请购文件","套",1,"成套供货，包括粉碎机和真空上料机","询比"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}