{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet15"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet15","index":0,"n_rows":26,"n_cols":7,"rows_kept":26,"merged":[[0,0,0,7],[1,6,1,7],[2,0,16,0],[2,1,3,1],[2,6,2,7],[3,6,3,7],[4,1,5,1],[4,6,4,7],[5,6,5,7],[6,1,7,1],[6,6,6,7],[7,6,7,7],[8,6,8,7],[9,6,9,7],[10,1,11,1],[10,2,11,2],[10,3,11,3],[10,4,11,4],[10,5,11,5],[10,6,10,7],[11,6,11,7],[12,6,12,7],[13,1,14,1],[13,2,14,2],[13,3,14,3],[13,4,14,4],[13,5,14,5],[13,6,13,7],[14,6,14,7],[15,1,16,1],[15,6,15,7],[16,6,16,7],[17,6,17,7],[18,6,18,7],[19,6,19,7],[20,1,20,6],[21,1,21,6],[22,1,22,6],[23,1,23,6],[24,1,24,6],[25,1,25,6],[27,0,27,7],[28,0,28,7]]}
["重庆聚狮新材料科技有限公司\n2025年自行监测报价单"]
["样品类型","点位","检测项目","分析费","频次","备注","总费用(元）"]
["有组织废气","缩合废气排放口（DA002）","硫化氢、氯苯类、",null,2,"1次/半年"]
[null,null,"烟气参数、挥发性有机物",null,12,"1次/月"]
[null,"焚烧炉废气排放口（DA004）","烟气参数、林格曼黑度、镉及其化合物、铅及其化合物、汞及其化合物、氨(氨气)、氮氧化物、一氧化碳、氯化氢、二氧化硫、颗粒物、铬，锡及其化合物、锑，铜，锰，砷及其化合物、镍及其化合物、钴",null,12,"1次/月"]
[null,null,"二噁英",null,1,"1次/年"]
[null,"污水处理站臭气排放口(DA006)","臭气浓度",null,2,"1次/半年"]
[null,null,"烟气参数、挥发性有机物",null,12,"1次/月"]
[null,"酸溶解废气排放口（DA008）","烟气参数、氯化氢",null,2,"1次/半年"]
[null,"破碎废气排放口 （DA010）","烟气参数、颗粒物",null,12,"1次/月"]
[null,"原料库废气排放口（DA012）","烟气参数、氯苯类",null,3,"1次/半年"]
[]
[null,"溶剂回收废气排放口（DA014）","烟气参数、挥发性有机物",null,12,"1次/月"]
[null,"干燥废气排放口（DA015）","烟气参数、氯苯类",null,3,"1次/半年"]
[]
[null,"无组织废气收集排放口（DA022）","非甲烷总烃、颗粒物",null,12,"1次/月"]
[null,null,"氯苯类",null,null,"1次/半年"]
["废水","废水处理站外排口（DW001）","总有机碳、硫化物、石油类、对二氯苯、可吸附卤化物",null,null,"1次/季度"]
["无组织废气","厂界","氨（氨气\n）、氯化氢、臭气浓度、硫化氢、颗粒物、非甲烷总烃、氯苯类",null,null,"1次/季度"]
["噪声","2个点位","昼间、夜间",null,null,"1次/季度"]
["检测费合计"]
["人员"]
["车辆"]
["税费","6%增值税专用发票"]
["合计","本次报价含3次免费复测费用"]
["最终报价"]